**SUGGESTED MEASURES FOR COMPONENTS WITH LEAD BASED PAINT**

|  |  |
| --- | --- |
| **Component with Positive XRF Reading**  | **Measure** |
|  Friction or impact surface (intact or deteriorated) |  Strip to bare wood and repaint or remove and replace.Baseboards can be stabilized and encapsulated. |
|   Non-friction or impact surface (door and window  trim, etc.) with deteriorated paint. |  Stabilize paint surface (wet sand/scrape) and repaint using approved encapsulation paint.  |
| Non-friction or impact surface (door and window  trim, etc.) with intact paint. | Technically, these surfaces do not require treatment, *except in an abatement.* However, we recommend "encapsulation" if the costs allow for it. |
|   Stair tread or riser.  | Strip to bare wood and repaint, remove and replace or enclose. |
|   Exterior windowsill  | Strip to bare wood and repaint, remove/replace or enclose. |
|   Interior windowsill  |  Strip to bare wood and repaint or remove and replace. |